<metadata>
	<idinfo>
		<citation>
			<citeinfo>
				<pubdate>20170601</pubdate>
				<title>elev_798_8</title>
				<geoform>raster digital data</geoform>
			</citeinfo>
		</citation>
		<descript>
			<abstract>Depth grids corresponding to mapped inundation areas from action stage through at least the flood of record for the Fox River at Waukesha, WI, NWSLI ID: WKEW3 and USGS ID: 05543830. The Flood Inundation Map Graphics show the lateral extent of projected flooding on local map backgrounds.</abstract>
			<purpose>This data set was developed exclusively for use with the National Weather Service's (NWS) Advanced Hydrologic Prediction Service (AHPS) website.</purpose>
			<supplinf>The initial target audience is the state and local agencies that must make emergency operational decisions during flooding events. However, since the graphics are easy to view, anyone with an interest during these events can make use of the maps, including the Federal Emergency Management Agency (FEMA), the U.S. Geological Survey (USGS), Corps of Engineers (COE), state and local emergency managers, the media, and the general public.</supplinf>
		</descript>
		<timeperd>
			<timeinfo>
				<sngdate>
					<caldate>20170601</caldate>
				</sngdate>
			</timeinfo>
			<current>publication date</current>
		</timeperd>
		<spdom>
			<bounding>
				<westbc>-88.270983</westbc>
				<eastbc>-88.207980</eastbc>
				<northbc>43.041403</northbc>
				<southbc>42.981239</southbc>
			</bounding>
		</spdom>
		<keywords>
			<theme>
				<themekt>None</themekt>
				<themekey>hydrologic prediction</themekey>
				<themekey>flood</themekey>
				<themekey>hydraulic</themekey>
				<themekey>flood inundation mapping</themekey>
				<themekey>modeling</themekey>
			</theme>
			<place>
				<placekt>None</placekt>
				<placekey>Fox River</placekey>
				<placekey>City of Waukesha</placekey>
				<placekey>Waukesha County</placekey>
				<placekey>Wisconsin</placekey>
			</place>
		</keywords>
		<accconst>The initial target audience is the state and local agencies that must make emergency operational decisions during flooding events. However, since the graphics are easy to view, anyone with an interest during these events can make use of the maps, including the Federal Emergency Management Agency (FEMA), the U.S. Geological Survey (USGS), Corps of Engineers (COE), state and local emergency managers, the media, and the general public.</accconst>
		<useconst>Users must assume responsibility to determine the appropriate use of this data. Users should be aware of the limitations of this dataset if using for critical application. Flood Inundation Maps will show the extent of flooding expected spatially over a given area. This will indicate when roadways, streets, buildings, airports, etc. are likely to be impacted by floodwaters. The accuracy of the mapping depends on the degree of accuracy of DEM data available for use in the GIS application, plus other factors. NOTE - The map layers for the 12.0 ft stage level indicate flooding of the quarry west of the river near Bluemound Road. This does not consider any local flood-fighting efforts. To keep the color scale reasonable for the rest of the map, the depth grids within the quarry are capped at the depth of the deepest flooding elsewhere. Should the quarry actually be flooded, depths will be significantly greater than depicted in the depth grid layer.</useconst>
		<ptcontac>
			<cntinfo>
				<cntorgp>
					<cntorg>Wisconsin Department of Natural Resources</cntorg>
				</cntorgp>
				<cntpos>Dams and Floodplain Section, Watershed Bureau</cntpos>
				<cntaddr>
					<addrtype>physical</addrtype>
					<address>101 South Webster Street</address>
					<city>Madison</city>
					<state>WI</state>
					<postal>53703</postal>
					<country>US</country>
				</cntaddr>
				<cntvoice>608-266-7014</cntvoice>
				<cntemail>Meg.Galloway@Wisconsin.gov</cntemail>
				<cntinst>Comments regarding the Flood Inundation Maps can be made here (http://www.weather.gov/survey/nws-survey.php?code=inundate)</cntinst>
			</cntinfo>
		</ptcontac>
		<datacred>The Wisconsin Department of Natural Resources (WDNR) conducted the hydraulic analysis and GIS analysis to produce the inundation data. NWS provided the QA\QC review of the data. Funding was received from FEMA for this project.</datacred>
		<native>Microsoft Windows 7 Version 6.1 (Build 7601) Service Pack 1; Esri ArcGIS 10.4.1.5686</native>
	</idinfo>
	<dataqual>
		<posacc>
			<horizpa>
				<horizpar>As with any engineering analysis of this type, variation from the estimated flood heights and floodplain boundaries is possible. Details of the process used to produce this data can be found in project documentation available from the data contact person. Horizontal accuracy was tested by evaluating boundaries to best available topographic dataset.</horizpar>
			</horizpa>
			<vertacc>
				<vertaccr>As with any engineering analysis of this type, variation from the estimated flood heights and floodplain boundaries is possible. Details of the process used to produce this data can be found in project documentation available from the data contact person. Vertical accuracy was tested by evaluating boundaries to best available topographic dataset.</vertaccr>
			</vertacc>
		</posacc>
	</dataqual>
	<spdoinfo>
		<direct>Raster</direct>
		<rastinfo>
			<rasttype>Grid Cell</rasttype>
			<rowcount>6010</rowcount>
			<colcount>4602</colcount>
		</rastinfo>
	</spdoinfo>
	<spref>
		<horizsys>
			<planar>
				<mapproj>
					<mapprojp>
						<otherprj>PROJCS["WGS_1984_Web_Mercator_Auxiliary_Sphere",GEOGCS["GCS_WGS_1984",DATUM["D_WGS_1984",SPHEROID["WGS_1984",6378137.0,298.257223563]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]],PROJECTION["Mercator_Auxiliary_Sphere"],PARAMETER["False_Easting",0.0],PARAMETER["False_Northing",0.0],PARAMETER["Central_Meridian",0.0],PARAMETER["Standard_Parallel_1",0.0],PARAMETER["Auxiliary_Sphere_Type",0.0],UNIT["Meter",1.0],AUTHORITY["EPSG",3857]],VERTCS["NAVD_1988_Foot_US",VDATUM["North_American_Vertical_Datum_1988"],PARAMETER["Vertical_Shift",0.0],PARAMETER["Direction",1.0],UNIT["Foot_US",0.3048006096012192],AUTHORITY["Esri",105703]]</otherprj>
					</mapprojp>
				</mapproj>
				<planci>
					<plance>coordinate pair</plance>
					<coordrep>
						<absres>0.000000006714873101998366</absres>
						<ordres>0.000000006714873101998366</ordres>
					</coordrep>
					<plandu>meter</plandu>
				</planci>
			</planar>
			<geodetic>
				<horizdn>D WGS 1984</horizdn>
				<ellips>WGS 1984</ellips>
				<semiaxis>6378137.0</semiaxis>
				<denflat>298.257223563</denflat>
			</geodetic>
		</horizsys>
		<vertdef>
			<altsys>
				<altdatum>North American Vertical Datum of 1988</altdatum>
				<altunits>feet</altunits>
			</altsys>
		</vertdef>
	</spref>
	<eainfo>
		<detailed>
			<enttyp>
				<enttypl>study_area</enttypl>
			</enttyp>
			<attr>
				<attrlabl>Shape</attrlabl>
				<attrdef>Feature geometry.</attrdef>
				<attrdefs>Esri</attrdefs>
				<attrdomv>
					<udom>Coordinates defining the features.</udom>
				</attrdomv>
			</attr>
			<attr>
				<attrlabl>FID</attrlabl>
				<attrdef>Internal feature number.</attrdef>
				<attrdefs>Esri</attrdefs>
				<attrdomv>
					<udom>Sequential unique whole numbers that are automatically generated.</udom>
				</attrdomv>
			</attr>
			<attr>
				<attrlabl>Id</attrlabl>
			</attr>
		</detailed>
	</eainfo>
	<metainfo>
		<metd>20170613</metd>
		<metstdn>FGDC Content Standard for Digital Geospatial Metadata</metstdn>
		<metstdv>FGDC-STD-001-1998</metstdv>
		<mettc>local time</mettc>
	</metainfo>
</metadata>
